simpleType networkModeChoices

type | restriction of xs:NMTOKEN
properties |
base | xs:NMTOKEN
used by |
attributes | EspduTransform/@networkMode ReceiverPdu/@networkMode SignalPdu/@networkMode TransmitterPdu/@networkMode
facets |
Kind | Value | Annotation
enumeration | standAlone |
appinfo
ignore network but still respond to events in local scene
enumeration | networkReader |
appinfo
listen to network and read PDU packets at readInterval, act as remotely linked copy of entity
enumeration | networkWriter |
appinfo
send PDU packets to network at writeInterval, act as master entity
annotation |
appinfo
networkModeChoices are strictly allowed enumeration values for DIS field networkMode. Bounded, no additional values are allowed.
source | <xs:simpleType name="networkModeChoices"> <xs:annotation> <xs:appinfo>networkModeChoices are strictly allowed enumeration values for DIS field networkMode. Bounded, no additional values are allowed.</xs:appinfo> <xs:documentation source="https://www.web3d.org/documents/specifications/19775-1/V3.3/Part01/components/dis.html#CommonDISfields"/> </xs:annotation> <xs:restriction base="xs:NMTOKEN"> <xs:enumeration value="standAlone"> <xs:annotation> <xs:appinfo>ignore network but still respond to events in local scene</xs:appinfo> </xs:annotation> </xs:enumeration> <xs:enumeration value="networkReader"> <xs:annotation> <xs:appinfo>listen to network and read PDU packets at readInterval, act as remotely linked copy of entity</xs:appinfo> </xs:annotation> </xs:enumeration> <xs:enumeration value="networkWriter"> <xs:annotation> <xs:appinfo>send PDU packets to network at writeInterval, act as master entity</xs:appinfo> </xs:annotation> </xs:enumeration> </xs:restriction> </xs:simpleType>

XML Schema documentation generated by XMLSpy Schema Editor http://www.altova.com/xmlspy