element TransmitterPdu

diagram |
type | extension of X3DNetworkSensorNode
properties |
content | complex
children | IS MetadataDouble MetadataFloat MetadataInteger MetadataSet MetadataString
used by |
group | ChildContentModelDIS
attributes |
Name | Type | Use | Default | Fixed | Annotation
DEF | xs:ID |  |  |  |
appinfo
DEF defines a unique ID name for each node, referenceable by other nodes.
USE | xs:IDREF |  |  |  |
appinfo
USE means reuse an already DEF-ed node ID, excluding all child nodes and all other attributes (except for containerField, which can have a different value).
class | xs:NMTOKENS |  |  |  |
appinfo
The class attribute is a space-separated list of classes, reserved for use by Cascading Style Sheets (CSS) and XML stylesheets.
enabled | SFBool |  | true |  |
bboxCenter | SFVec3f |  | 0 0 0 |  |
bboxSize | bboxSizeType |  | -1 -1 -1 |  |
whichGeometry | SFInt32 |  | 1 |  |
readInterval | derived by: SFTime |  | 0.1 |  |
writeInterval | derived by: SFTime |  | 1.0 |  |
networkMode | networkModeChoices |  | standAlone |  |
siteID | SFInt32 |  | 0 |  |
applicationID | SFInt32 |  | 0 |  |
entityID | SFInt32 |  | 0 |  |
address | SFString |  | localhost |  |
port | SFInt32 |  | 0 |  |
multicastRelayHost | SFString |  |  |  |
multicastRelayPort | SFInt32 |  | 0 |  |
rtpHeaderExpected | SFBool |  | false |  |
radioID | SFInt32 |  | 0 |  |
antennaLocation | SFVec3f |  | 0 0 0 |  |
antennaPatternLength | SFInt32 |  | 0 |  |
antennaPatternType | SFInt32 |  | 0 |  |
cryptoKeyID | SFInt32 |  | 0 |  |
cryptoSystem | SFInt32 |  | 0 |  |
frequency | SFInt32 |  | 0 |  |
inputSource | SFInt32 |  | 0 |  |
lengthOfModulationParameters | SFInt32 |  | 0 |  |
modulationTypeDetail | SFInt32 |  | 0 |  |
modulationTypeMajor | SFInt32 |  | 0 |  |
modulationTypeSpreadSpectrum | SFInt32 |  | 0 |  |
modulationTypeSystem | SFInt32 |  | 0 |  |
power | SFFloat |  | 0.0 |  |
radioEntityTypeCategory | SFInt32 |  | 0 |  |
radioEntityTypeCountry | SFInt32 |  | 0 |  |
radioEntityTypeDomain | SFInt32 |  | 0 |  |
radioEntityTypeKind | SFInt32 |  | 0 |  |
radioEntityTypeNomenclature | SFInt32 |  | 0 |  |
radioEntityTypeNomenclatureVersion | SFInt32 |  | 0 |  |
relativeAntennaLocation | SFVec3f |  | 0 0 0 |  |
transmitFrequencyBandwidth | SFFloat |  | 0 |  |
transmitState | SFInt32 |  | 0 |  |
geoSystem | geoSystemType |  | "GD" "WE" |  |
geoCoords | SFVec3d |  | 0 0 0 |  |
containerField | xs:NMTOKEN |  | children |  |
annotation |
appinfo
<xs:attribute name="isNetworkReader" type="SFBool" fixed="outputOnlyField"/> <xs:attribute name="isNetworkWriter" type="SFBool" fixed="outputOnlyField"/> <xs:attribute name="isRtpHeaderHeard" type="SFBool" fixed="outputOnlyField"/> <xs:attribute name="isStandAlone" type="SFBool" fixed="outputOnlyField"/> <xs:attribute name="timestamp" fixed="outputOnlyField"> <!-- type="SFTimeNonNegative" --> <xs:simpleType> <xs:restriction base="SFTime"> <xs:minInclusive value="0"/> </xs:restriction> </xs:simpleType> </xs:attribute> <xs:attribute name="additionalInterface" type="xs:string" default="X3DBoundedObject"/> <xs:attribute name="componentName" type="componentNameChoices" fixed="DIS"/> <xs:attribute name="componentLevel" type="xs:positiveInteger" fixed="1"/>
source | <xs:element name="TransmitterPdu"> <xs:annotation> <xs:appinfo> <xs:attribute name="isNetworkReader" type="SFBool" fixed="outputOnlyField"/> <xs:attribute name="isNetworkWriter" type="SFBool" fixed="outputOnlyField"/> <xs:attribute name="isRtpHeaderHeard" type="SFBool" fixed="outputOnlyField"/> <xs:attribute name="isStandAlone" type="SFBool" fixed="outputOnlyField"/> <xs:attribute name="timestamp" fixed="outputOnlyField"> <!-- type="SFTimeNonNegative" --> <xs:simpleType> <xs:restriction base="SFTime"> <xs:minInclusive value="0"/> </xs:restriction> </xs:simpleType> </xs:attribute> <xs:attribute name="additionalInterface" type="xs:string" default="X3DBoundedObject"/> <xs:attribute name="componentName" type="componentNameChoices" fixed="DIS"/> <xs:attribute name="componentLevel" type="xs:positiveInteger" fixed="1"/> </xs:appinfo> <xs:documentation source="https://www.web3d.org/documents/specifications/19775-1/V3.3/Part01/components/dis.html#TransmitterPdu"/> </xs:annotation> <xs:complexType> <xs:complexContent> <xs:extension base="X3DNetworkSensorNode"> <xs:attribute name="bboxCenter" type="SFVec3f" default="0 0 0"/> <xs:attribute name="bboxSize" type="bboxSizeType" default="-1 -1 -1"/> <xs:attribute name="whichGeometry" type="SFInt32" default="1"/> <xs:attribute name="readInterval" default="0.1"> <!-- type="SFTimeNonNegative" --> <xs:simpleType> <xs:restriction base="SFTime"> <xs:minInclusive value="0"/> </xs:restriction> </xs:simpleType> </xs:attribute> <xs:attribute name="writeInterval" default="1.0"> <!-- type="SFTimeNonNegative" --> <xs:simpleType> <xs:restriction base="SFTime"> <xs:minInclusive value="0"/> </xs:restriction> </xs:simpleType> </xs:attribute> <xs:attribute name="networkMode" type="networkModeChoices" default="standAlone"/> <xs:attribute name="siteID" type="SFInt32" default="0"/> <xs:attribute name="applicationID" type="SFInt32" default="0"/> <xs:attribute name="entityID" type="SFInt32" default="0"/> <xs:attribute name="address" type="SFString" default="localhost"/> <xs:attribute name="port" type="SFInt32" default="0"/> <xs:attribute name="multicastRelayHost" type="SFString"/> <xs:attribute name="multicastRelayPort" type="SFInt32" default="0"/> <xs:attribute name="rtpHeaderExpected" type="SFBool" default="false"/> <xs:attribute name="radioID" type="SFInt32" default="0"/> <xs:attribute name="antennaLocation" type="SFVec3f" default="0 0 0"/> <xs:attribute name="antennaPatternLength" type="SFInt32" default="0"/> <xs:attribute name="antennaPatternType" type="SFInt32" default="0"/> <xs:attribute name="cryptoKeyID" type="SFInt32" default="0"/> <xs:attribute name="cryptoSystem" type="SFInt32" default="0"/> <xs:attribute name="frequency" type="SFInt32" default="0"/> <xs:attribute name="inputSource" type="SFInt32" default="0"/> <xs:attribute name="lengthOfModulationParameters" type="SFInt32" default="0"/> <xs:attribute name="modulationTypeDetail" type="SFInt32" default="0"/> <xs:attribute name="modulationTypeMajor" type="SFInt32" default="0"/> <xs:attribute name="modulationTypeSpreadSpectrum" type="SFInt32" default="0"/> <xs:attribute name="modulationTypeSystem" type="SFInt32" default="0"/> <xs:attribute name="power" type="SFFloat" default="0.0"/> <xs:attribute name="radioEntityTypeCategory" type="SFInt32" default="0"/> <xs:attribute name="radioEntityTypeCountry" type="SFInt32" default="0"/> <xs:attribute name="radioEntityTypeDomain" type="SFInt32" default="0"/> <xs:attribute name="radioEntityTypeKind" type="SFInt32" default="0"/> <xs:attribute name="radioEntityTypeNomenclature" type="SFInt32" default="0"/> <xs:attribute name="radioEntityTypeNomenclatureVersion" type="SFInt32" default="0"/> <xs:attribute name="relativeAntennaLocation" type="SFVec3f" default="0 0 0"/> <xs:attribute name="transmitFrequencyBandwidth" type="SFFloat" default="0"/> <xs:attribute name="transmitState" type="SFInt32" default="0"/> <xs:attribute name="geoSystem" type="geoSystemType" default='"GD" "WE"'/> <xs:attribute name="geoCoords" type="SFVec3d" default="0 0 0"/> <xs:attribute name="containerField" type="xs:NMTOKEN" default="children"/> </xs:extension> <!-- bboxDisplay, visible added in X3D version 4.0 --> </xs:complexContent> </xs:complexType> </xs:element>

attribute TransmitterPdu/@bboxCenter

type | SFVec3f
properties |
default | 0 0 0
facets |
Kind | Value | Annotation
whiteSpace | collapse |
pattern | \s*(([+-]?((0|[1-9][0-9]*)(\.[0-9]*)?|\.[0-9]+)([Ee][+-]?[0-9]+)?)\s+){2}([+-]?((0|[1-9][0-9]*)(\.[0-9]*)?|\.[0-9]+)([Ee][+-]?[0-9]+)?)\s* |
source | <xs:attribute name="bboxCenter" type="SFVec3f" default="0 0 0"/>

attribute TransmitterPdu/@bboxSize

type | bboxSizeType
properties |
default | -1 -1 -1
facets |
Kind | Value | Annotation
whiteSpace | collapse |
pattern | \s*((([+]?(((0|[1-9][0-9]*)(\.[0-9]*)?|\.[0-9]+)([Ee][+-]?[0-9]+)?)\s+){2}([+]?((0|[1-9][0-9]*)(\.[0-9]*)?|\.[0-9]+)([Ee][+-]?[0-9]+)?)\s*)|((\-1(\.(0)*)?([Ee][+-]?[0]+)?\s+){2}\-1(\.(0)*)?([Ee][+-]?[0]+)?)\s*)? |
source | <xs:attribute name="bboxSize" type="bboxSizeType" default="-1 -1 -1"/>

attribute TransmitterPdu/@whichGeometry

type | SFInt32
properties |
default | 1
source | <xs:attribute name="whichGeometry" type="SFInt32" default="1"/>

attribute TransmitterPdu/@readInterval

type | restriction of SFTime
properties |
default | 0.1
facets |
Kind | Value | Annotation
minInclusive | 0 |
source | <xs:attribute name="readInterval" default="0.1"> <!-- type="SFTimeNonNegative" --> <xs:simpleType> <xs:restriction base="SFTime"> <xs:minInclusive value="0"/> </xs:restriction> </xs:simpleType> </xs:attribute>

attribute TransmitterPdu/@writeInterval

type | restriction of SFTime
properties |
default | 1.0
facets |
Kind | Value | Annotation
minInclusive | 0 |
source | <xs:attribute name="writeInterval" default="1.0"> <!-- type="SFTimeNonNegative" --> <xs:simpleType> <xs:restriction base="SFTime"> <xs:minInclusive value="0"/> </xs:restriction> </xs:simpleType> </xs:attribute>

attribute TransmitterPdu/@networkMode

type | networkModeChoices
properties |
default | standAlone
facets |
Kind | Value | Annotation
enumeration | standAlone |
appinfo
ignore network but still respond to events in local scene
enumeration | networkReader |
appinfo
listen to network and read PDU packets at readInterval, act as remotely linked copy of entity
enumeration | networkWriter |
appinfo
send PDU packets to network at writeInterval, act as master entity
source | <xs:attribute name="networkMode" type="networkModeChoices" default="standAlone"/>

attribute TransmitterPdu/@siteID

type | SFInt32
properties |
default | 0
source | <xs:attribute name="siteID" type="SFInt32" default="0"/>

attribute TransmitterPdu/@applicationID

type | SFInt32
properties |
default | 0
source | <xs:attribute name="applicationID" type="SFInt32" default="0"/>

attribute TransmitterPdu/@entityID

type | SFInt32
properties |
default | 0
source | <xs:attribute name="entityID" type="SFInt32" default="0"/>

attribute TransmitterPdu/@address

type | SFString
properties |
default | localhost
source | <xs:attribute name="address" type="SFString" default="localhost"/>

attribute TransmitterPdu/@port

type | SFInt32
properties |
default | 0
source | <xs:attribute name="port" type="SFInt32" default="0"/>

attribute TransmitterPdu/@multicastRelayHost

type | SFString
source | <xs:attribute name="multicastRelayHost" type="SFString"/>

attribute TransmitterPdu/@multicastRelayPort

type | SFInt32
properties |
default | 0
source | <xs:attribute name="multicastRelayPort" type="SFInt32" default="0"/>

attribute TransmitterPdu/@rtpHeaderExpected

type | SFBool
properties |
default | false
source | <xs:attribute name="rtpHeaderExpected" type="SFBool" default="false"/>

attribute TransmitterPdu/@radioID

type | SFInt32
properties |
default | 0
source | <xs:attribute name="radioID" type="SFInt32" default="0"/>

attribute TransmitterPdu/@antennaLocation

type | SFVec3f
properties |
default | 0 0 0
facets |
Kind | Value | Annotation
whiteSpace | collapse |
pattern | \s*(([+-]?((0|[1-9][0-9]*)(\.[0-9]*)?|\.[0-9]+)([Ee][+-]?[0-9]+)?)\s+){2}([+-]?((0|[1-9][0-9]*)(\.[0-9]*)?|\.[0-9]+)([Ee][+-]?[0-9]+)?)\s* |
source | <xs:attribute name="antennaLocation" type="SFVec3f" default="0 0 0"/>

attribute TransmitterPdu/@antennaPatternLength

type | SFInt32
properties |
default | 0
source | <xs:attribute name="antennaPatternLength" type="SFInt32" default="0"/>

attribute TransmitterPdu/@antennaPatternType

type | SFInt32
properties |
default | 0
source | <xs:attribute name="antennaPatternType" type="SFInt32" default="0"/>

attribute TransmitterPdu/@cryptoKeyID

type | SFInt32
properties |
default | 0
source | <xs:attribute name="cryptoKeyID" type="SFInt32" default="0"/>

attribute TransmitterPdu/@cryptoSystem

type | SFInt32
properties |
default | 0
source | <xs:attribute name="cryptoSystem" type="SFInt32" default="0"/>

attribute TransmitterPdu/@frequency

type | SFInt32
properties |
default | 0
source | <xs:attribute name="frequency" type="SFInt32" default="0"/>

attribute TransmitterPdu/@inputSource

type | SFInt32
properties |
default | 0
source | <xs:attribute name="inputSource" type="SFInt32" default="0"/>

attribute TransmitterPdu/@lengthOfModulationParameters

type | SFInt32
properties |
default | 0
source | <xs:attribute name="lengthOfModulationParameters" type="SFInt32" default="0"/>

attribute TransmitterPdu/@modulationTypeDetail

type | SFInt32
properties |
default | 0
source | <xs:attribute name="modulationTypeDetail" type="SFInt32" default="0"/>

attribute TransmitterPdu/@modulationTypeMajor

type | SFInt32
properties |
default | 0
source | <xs:attribute name="modulationTypeMajor" type="SFInt32" default="0"/>

attribute TransmitterPdu/@modulationTypeSpreadSpectrum

type | SFInt32
properties |
default | 0
source | <xs:attribute name="modulationTypeSpreadSpectrum" type="SFInt32" default="0"/>

attribute TransmitterPdu/@modulationTypeSystem

type | SFInt32
properties |
default | 0
source | <xs:attribute name="modulationTypeSystem" type="SFInt32" default="0"/>

attribute TransmitterPdu/@power

type | SFFloat
properties |
default | 0.0
source | <xs:attribute name="power" type="SFFloat" default="0.0"/>

attribute TransmitterPdu/@radioEntityTypeCategory

type | SFInt32
properties |
default | 0
source | <xs:attribute name="radioEntityTypeCategory" type="SFInt32" default="0"/>

attribute TransmitterPdu/@radioEntityTypeCountry

type | SFInt32
properties |
default | 0
source | <xs:attribute name="radioEntityTypeCountry" type="SFInt32" default="0"/>

attribute TransmitterPdu/@radioEntityTypeDomain

type | SFInt32
properties |
default | 0
source | <xs:attribute name="radioEntityTypeDomain" type="SFInt32" default="0"/>

attribute TransmitterPdu/@radioEntityTypeKind

type | SFInt32
properties |
default | 0
source | <xs:attribute name="radioEntityTypeKind" type="SFInt32" default="0"/>

attribute TransmitterPdu/@radioEntityTypeNomenclature

type | SFInt32
properties |
default | 0
source | <xs:attribute name="radioEntityTypeNomenclature" type="SFInt32" default="0"/>

attribute TransmitterPdu/@radioEntityTypeNomenclatureVersion

type | SFInt32
properties |
default | 0
source | <xs:attribute name="radioEntityTypeNomenclatureVersion" type="SFInt32" default="0"/>

attribute TransmitterPdu/@relativeAntennaLocation

type | SFVec3f
properties |
default | 0 0 0
facets |
Kind | Value | Annotation
whiteSpace | collapse |
pattern | \s*(([+-]?((0|[1-9][0-9]*)(\.[0-9]*)?|\.[0-9]+)([Ee][+-]?[0-9]+)?)\s+){2}([+-]?((0|[1-9][0-9]*)(\.[0-9]*)?|\.[0-9]+)([Ee][+-]?[0-9]+)?)\s* |
source | <xs:attribute name="relativeAntennaLocation" type="SFVec3f" default="0 0 0"/>

attribute TransmitterPdu/@transmitFrequencyBandwidth

type | SFFloat
properties |
default | 0
source | <xs:attribute name="transmitFrequencyBandwidth" type="SFFloat" default="0"/>

attribute TransmitterPdu/@transmitState

type | SFInt32
properties |
default | 0
source | <xs:attribute name="transmitState" type="SFInt32" default="0"/>

attribute TransmitterPdu/@geoSystem

type | geoSystemType
properties |
default | "GD" "WE"
source | <xs:attribute name="geoSystem" type="geoSystemType" default='"GD" "WE"'/>

attribute TransmitterPdu/@geoCoords

type | SFVec3d
properties |
default | 0 0 0
facets |
Kind | Value | Annotation
whiteSpace | collapse |
pattern | \s*(([+-]?((0|[1-9][0-9]*)(\.[0-9]*)?|\.[0-9]+)([Ee][+-]?[0-9]+)?)\s+){2}([+-]?((0|[1-9][0-9]*)(\.[0-9]*)?|\.[0-9]+)([Ee][+-]?[0-9]+)?)\s* |
source | <xs:attribute name="geoCoords" type="SFVec3d" default="0 0 0"/>

attribute TransmitterPdu/@containerField

type | xs:NMTOKEN
properties |
default | children
source | <xs:attribute name="containerField" type="xs:NMTOKEN" default="children"/>

XML Schema documentation generated by XMLSpy Schema Editor http://www.altova.com/xmlspy